**Scan Continuous Tone-Coded Squelch:**

1. **Between CH 1-22 & CTCS 0-38**
2. **Turn on “Channel mode”**
3. **Copy frequency of the channel**
4. **Go to “Frequency mode”**
5. **Set the frequency manually**
6. **Go to menu 11 (R-CTCS)**
7. **Set any CTCS and press SCAN**
8. **Transmit with the other radio**
9. **The handset will stop into the right CTCS**
10. **Set on menu 11 & 13 the right CTCS**
11. **Go to menu 27 and save CH-0 memory**
12. **Turn on “Channel mode” and use de saved one**